TV power button
show_name: true
show_icon: true
type: button
tap_action:
  action: call-service
  service: mqtt.publish
  data:
    topic: cmnd/ir/IRSend
    payload: '{"protocol": "NEC","bits": 32, "data": 0x20DF10EF}'
  target: {}
icon: mdi:television