Contents: [Dobrica Pavlinušić's random unstructured stuff]
• Dobrica Pavlinušić's random unstructured stuff (u‑boot) 
• Dobrica Pavlinušić's random unstructured stuff (Info) 
• Dobrica Pavlinušić's random unstructured stuff (dfu‑util) 
• Dobrica Pavlinušić's random unstructured stuff (flash kernel) 
• Dobrica Pavlinušić's random unstructured stuff (flash rootfs) 
• Dobrica Pavlinušić's random unstructured stuff (openocd) 
• Dobrica Pavlinušić's random unstructured stuff (Android) 
• Dobrica Pavlinušić's random unstructured stuff (Open Issues) 
• Dobrica Pavlinušić's random unstructured stuff (Pending issues) 
• Dobrica Pavlinušić's random unstructured stuff (Resolved issues) 
• Dobrica Pavlinušić's random unstructured stuff (Qemu) 
• Dobrica Pavlinušić's random unstructured stuff (See also) 
• Dobrica Pavlinušić's random unstructured stuff (Other pages on this wiki about OpenMoko) 
• Dobrica Pavlinušić's random unstructured stuff (My blog posts about OpenMoko) 

u‑boot
• http://wiki.openmoko.org/wiki/NeoCon 
• http://wiki.openmoko.org/wiki/NAND_bad_blocks 
Recover from bad blocks procedure
x200:/virtual/openmoko# ./neocon/neocon /dev/ttyACM*
[Open /dev/ttyACM3]
In:    usbtty
Out:   usbtty
Err:   usbtty
DEVICE_CONFIGURED: 1
Enabling automatic fast charge

GTA01Bv4 # nand bad

Device 0 bad blocks:
  00070000
  00ab0000
  00f00000
  03ff0000
  03ff4000
  03ff8000
  03ffc000

GTA01Bv4 # nand scrub

NAND scrub: device 0 whole chip
Warning: scrub option will erase all factory set bad blocks!
         There is no reliable way to recover them.
         Use this command only for testing purposes if you
         are sure of what you are doing!

Really scrub this NAND flash? <y/N>

NAND 64MiB 3,3V 8-bit: MTD Erase failure: -5

NAND 64MiB 3,3V 8-bit: MTD Erase failure: -5

NAND 64MiB 3,3V 8-bit: MTD Erase failure: -5
Bad block table not found for chip 0
Bad block table not found for chip 0
OK

GTA01Bv4 # nand createbbt
Create BBT and erase everything ? <y/N>
Skipping bad block at  0x00070000                                            
Skipping bad block at  0x00ab0000                                            
Skipping bad block at  0x00f00000                                            
Skipping bad block at  0x03ff0000                                            
Skipping bad block at  0x03ff4000                                            
Skipping bad block at  0x03ff8000                                            
Skipping bad block at  0x03ffc000                                            

Creating BBT. Please wait ...Bad block table not found for chip 0
Bad block table not found for chip 0
Bad block table written to 0x03ffc000, version 0x01
Bad block table written to 0x03ff8000, version 0x01

GTA01Bv4 # dynpart
mtdparts mtdparts=neo1973-nand:0x00040000(u-boot),0x00004000(u-boot_env),0x00204000(kernel),0x000a0000(splash),0x03d18000(rootfs)

GTA01Bv4 # dynenv set u-boot_env
device 0 offset 0x40000, size 0x4000
45 4e 56 30 - 00 00 04 00

GTA01Bv4 # saveenv
Saving Environment to NAND...
Saving ESaving EnvironmnvironmWriting to Nand... done

Info
GTA01Bv4 # bdinfo
arch_number = 0x0000049E
env_t       = 0x00000000
boot_params = 0x30000100
DRAM bank   = 0x00000000
-> start    = 0x30000000
-> size     = 0x08000000
ethaddr     = 00:00:00:00:00:00

ip_addr     = 0.0.0.0
baudrate    = 115200 bps

GTA01Bv4 # printenv
baudrate=115200
bootcmd=setenv bootargs ${bootargs_base} ${mtdparts}; nand read.e 0x32000000 kernel; bootm 0x32000000
bootdelay=1
menu_1=Set console to USB: setenv stdin usbtty; setenv stdout usbtty; setenv stderr usbtty
menu_2=Set console to serial: setenv stdin serial; setenv stdout serial; setenv stderr serial
menu_3=Power off: neo1973 power-off
menu_4=Boot from SD: setenv bootargs root=/dev/mmcblk0p1 rootdelay=5 console=ttySAC0,115200 console=tty0 loglevel=8 ${mtdparts} ro; mmcinit; ext2load mmc 0 0x32000000 /boot/${sd_image_name}; bootm 0x32000000
mtdids=nand0=neo1973-nand
quiet=1
sd_image_name=uImage
splashimage=nand read.e 0x32000000 splash 0x5000; unzip 0x32000000 0x33d00000 0x96000
stderr=usbtty
stdin=usbtty
stdout=usbtty
usbtty=cdc_acm
bootargs_base=rootfstype=jffs2 root=/dev/mtdblock4 console=tty0 loglevel=8
mtdparts=mtdparts=neo1973-nand:0x00040000(u-boot),0x00004000(u-boot_env),0x00204000(kernel),0x000a0000(splash),0x03d18000(rootfs)
mtdparts=mtdparts=nmtddevnum=0
mtddevname=u-boot
pcf50606_int1=0x4a

Environment size: 1028/16380 bytes

GTA01Bv4 # mtd

device nand0 <neo1973-nand>, # parts = 5
 #: name                        size            offset          mask_flags
 0: u-boot              0x00040000      0x00000000      0
 1: u-boot_env          0x00004000      0x00040000      0
 2: kernel              0x00204000      0x00044000      0
 3: splash              0x000a0000      0x00248000      0
 4: rootfs              0x03d18000      0x002e8000      0

active partition: nand0,0 - (u-boot) 0x00040000 @ 0x00000000

defaults:
mtdids  : nand0=neo1973-nand
mtdparts: <NULL>

dfu‑util
Disable bluetooth which also responds to dfu:
x200:/home/dpavlin# echo disable > /proc/acpi/ibm/bluetooth

• http://wiki.openmoko.org/wiki/Flashing_the_Neo_1973 
Boot moko by pressing AUX (top‑left smooth button) and power (on the right below usb cable)
x200:/virtual/openmoko# dfu-util --list
dfu-util - (C) 2007-2008 by OpenMoko Inc.
This program is Free Software and has ABSOLUTELY NO WARRANTY

dfu-util does currently only support DFU version 1.0

Found Runtime: [0x1457:0x5119] devnum=38, cfg=0, intf=2, alt=0, name="USB Device Firmware Upgrade"

Hm. We need to reset device in DFU mode
x200:/virtual/openmoko# dfu-util --device 0x1457:0x5119 --download xx
dfu-util - (C) 2007-2008 by OpenMoko Inc.
This program is Free Software and has ABSOLUTELY NO WARRANTY

dfu-util does currently only support DFU version 1.0

Opening USB Device 0x1457:0x5119...
Claiming USB DFU Runtime Interface...
Determining device status: state = appIDLE, status = 0
Device really in Runtime Mode, send DFU detach request...
Resetting USB...
Opening USB Device...
Found Runtime: [0x1457:0x5119] devnum=39, cfg=0, intf=0, alt=0, name="RAM 0x32000000"
We have 6 DFU Interfaces/Altsettings, you have to specify one via --intf / --alt options

x200:/virtual/openmoko# dfu-util --device 0x1457:0x5119 --list
dfu-util - (C) 2007-2008 by OpenMoko Inc.
This program is Free Software and has ABSOLUTELY NO WARRANTY

dfu-util does currently only support DFU version 1.0

Found DFU: [0x1457:0x5119] devnum=39, cfg=0, intf=0, alt=0, name="RAM 0x32000000"
Found DFU: [0x1457:0x5119] devnum=39, cfg=0, intf=0, alt=1, name="u-boot"
Found DFU: [0x1457:0x5119] devnum=39, cfg=0, intf=0, alt=2, name="u-boot_env"
Found DFU: [0x1457:0x5119] devnum=39, cfg=0, intf=0, alt=3, name="kernel"
Found DFU: [0x1457:0x5119] devnum=39, cfg=0, intf=0, alt=4, name="splash"
Found DFU: [0x1457:0x5119] devnum=39, cfg=0, intf=0, alt=5, name="rootfs"

flash kernel
x200:/virtual/openmoko/fso# dfu-util -a kernel -R -D uImage-2.6.24-oe5+gitrfb42ce6724576fc173faf8abfb04aa2c36d213b7-r1-om-gta01.bin 
dfu-util- (C) 2007-2008 by OpenMoko Inc.
This program is Free Software and has ABSOLUTELY NO WARRANTY

dfu-util does currently only support DFU version 1.0

Opening USB Device 0x0000:0x0000...
Found Runtime: [0x1457:0x5119] devnum=39, cfg=0, intf=0, alt=3, name="kernel"
Claiming USB DFU Interface...
Setting Alternate Setting #3 ...
Determining device status: state = dfuIDLE, status = 0
dfuIDLE, continuing
Transfer Size = 0x1000
bytes_per_hash=38298
Starting download: [##################################################] finished!
state(2) = dfuIDLE, status(0) = No error condition is present
Done!
Resetting USB to switch back to runtime mode

flash rootfs
x200:/virtual/openmoko/fso# dfu-util -a rootfs -R -D openmoko-fso-console-image-glibc-ipk--20090223-om-gta01.rootfs.jffs2 
dfu-util- (C) 2007-2008 by OpenMoko Inc.
This program is Free Software and has ABSOLUTELY NO WARRANTY

dfu-util does currently only support DFU version 1.0

Opening USB Device 0x0000:0x0000...
Found Runtime: [0x1457:0x5119] devnum=41, cfg=0, intf=0, alt=5, name="rootfs"
Claiming USB DFU Interface...
Setting Alternate Setting #5 ...
Determining device status: state = dfuERROR, status = 14
dfuERROR, clearing status
Determining device status: state = dfuIDLE, status = 0
dfuIDLE, continuing
Transfer Size = 0x1000
bytes_per_hash=452853
Starting download: [##################################################dfu_download: usb_control_msg returned -110: error sending control message: Connection timed out] finished!
unable to read DFU status

No worky
openocd
• openocd.cfg 
• http://wiki.openmoko.org/wiki/Neo1973_OpenOCD 
x200:/virtual/openmoko# openocd 
Open On-Chip Debugger 0.4.0 (2010-02-23-17:04)
Licensed under GNU GPL v2
For bug reports, read
        http://openocd.berlios.de/doc/doxygen/bugs.html
trst_and_srst separate srst_gates_jtag trst_push_pull srst_open_drain
trst_and_srst separate srst_gates_jtag trst_push_pull srst_open_drain
Info : clock speed 6000 kHz
Info : JTAG tap: s3c2440.cpu tap/device found: 0x0032409d (mfg: 0x04e, part: 0x0324, ver: 0x0)
Info : Embedded ICE version 2
Info : s3c2440.cpu: hardware has 2 breakpoint/watchpoint units
Info : JTAG tap: s3c2440.cpu tap/device found: 0x0032409d (mfg: 0x04e, part: 0x0324, ver: 0x0)
Warn : NOTE! DCC downloads have not been enabled, defaulting to slow memory writes. Type 'help dcc'.
Warn : NOTE! Severe performance degradation without fast memory access enabled. Type 'help fast'.
target state: halted
target halted in ARM state due to debug-request, current mode: Supervisor
cpsr: 0x20000053 pc: 0x33f966d8
MMU: disabled, D-Cache: enabled, I-Cache: enabled
Info : accepting 'telnet' connection from 0
Runtime error, file "command.c", line 650:
    invalid command name "run"
Info : JTAG tap: s3c2440.cpu tap/device found: 0x0032409d (mfg: 0x04e, part: 0x0324, ver: 0x0)
Warn : NOTE! DCC downloads have not been enabled, defaulting to slow memory writes. Type 'help dcc'.
Warn : NOTE! Severe performance degradation without fast memory access enabled. Type 'help fast'.

                                                  
Scratch pad for my notes about OpenMoko
Android
• http://onlinedev.blogspot.com/2008/11/porting‑android‑phase‑4‑done.html 
dpavlin@llin:/rest/cvs/qemu-neo1973/openmoko/android$ wget -r -np -m http://people.openmoko.org/sean_mcneil/

Open Issues
• how to start matchbox‑stroke  ?
• gsmd problem 
Pending issues
• gps driver 
• using keyboard without mouse ‑‑ Finger Keyboard 
Resolved issues
• correct time ‑‑ ipkg install ntpdate
Qemu
Alternative way to build qemu with Neo 1973 emulation:
# checkout source

svn co https://svn.openmoko.org/trunk/src/host/qemu-neo1973
cd qemu-neo1973

# run configure

./configure --target-list=arm-softmmu --enable-gadgetfs

# needed for gadgetfs to work

ln -s /usr/src/linux/include/linux

# build it

make

See also
Other pages on this wiki about OpenMoko

Search for openmoko 

• Ubertooth One 
• Android G1 
• OpenMoko 
• OpenMoko as a phone 
• OpenMoko arrived 

My blog posts about OpenMoko
Search Results for openmoko 
• OpenMoko GPS tracking 
• OpenMoko flashing 
• OpenMoko as a phone 
• OpenMoko arrived 
• OpenMoko paid 
• OpenMoko and why I ordered one 

.pre