My notes about compilation and usage

Contents: [Dobrica Pavlinušić's random unstructured stuff]
• Dobrica Pavlinušić's random unstructured stuff (Checkout source) 
• Dobrica Pavlinušić's random unstructured stuff (TP‑Link TL‑WR741ND) 
• Dobrica Pavlinušić's random unstructured stuff (TP‑Link TL‑WDR4300) 
• Dobrica Pavlinušić's random unstructured stuff (SIEMENS Gigaset SX763) 

Checkout source
dpavlin@blue:/bluez/openwrt$ git clone git://git.openwrt.org/openwrt.git

                                                  
Random notes about router unbricking
TP‑Link TL‑WR741ND

http://wiki.openwrt.org/toh/tp‑link/tl‑wr741nd 
for 4.24 download v4 image!
https://downloads.openwrt.org/snapshots/trunk/ar71xx/openwrt‑ar71xx‑generic‑tl‑wr741nd‑v4‑squashfs‑sysupgrade.bin 
tpl on "Autobooting in 1 seconds" prompt to get console.
ar7240> setenv ipaddr 10.0.0.100
ar7240> setenv serverip 10.0.0.1

ar7240> tftpboot 0x80000000 openwrt-ar71xx-generic-tl-wr741nd-v4-squashfs-sysupgrade.bin
dup 1 speed 1000
Using eth1 device
FTP from server 10.0.0.1; our IP address is 10.0.0.100
Filename 'openwrt-ar71xx-generic-tl-wr741nd-v2-squashfs-sysupgrade.bin'.
Load address: 0x80000000
Loading: #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################
done
Bytes transferred = 3080196 (2f0004 hex)

ar7240> erase 0x9f020000 +2f0004

First 0x2 last 0x31 sector size 0x10000
  49
Erased 48 sectors

ar7240> cp.b 0x80000000 0x9f020000 0x2f0004
Copy to Flash... write addr: 9f020000
done

ar7240> bootm 0x9f020000

TP‑Link TL‑WDR4300
http://wiki.openwrt.org/toh/tp‑link/tl‑wdr4300 
U-Boot 1.1.4 (Jun 17 2013 - 12:31:57)

U-boot DB120

DRAM:  128 MB
id read 0x100000ff
flash size 8MB, sector count = 128
Flash:  8 MB
Using default environment

PCIe Reset OK!!!!!!
In:    serial
Out:   serial
Err:   serial
Net:   ag934x_enet_initialize...
No valid address in Flash. Using fixed address
 wasp  reset mask:c03300 
WASP  ----> S17 PHY *
: cfg1 0x7 cfg2 0x7114
eth0: ba:be:fa:ce:08:41
athrs17_reg_init: complete
eth0 up
eth0
Autobooting in 1 seconds
db12x> 
db12x> 
db12x> setenv ipaddr 10.0.0.100
db12x> setenv serverip 10.0.0.1
db12x> 
db12x> tftpboot
dup 1 speed 1000
*** Warning: no boot file name; using '6F01A8C0.img'
Using eth0 device
TFTP from server 192.168.1.100; our IP address is 192.168.1.111
Filename '6F01A8C0.img'.
Load address: 0x81000000

root@blue:/srv/tftp# ln -s openwrt-ar71xx-generic-tl-wdr4300-v1-squashfs-sysupgrade.bin 6400000A.img

db12x> tftpboot
*** Warning: no boot file name; using '6400000A.img'
Using eth0 device
TFTP from server 10.0.0.1; our IP address is 10.0.0.100
Filename '6400000A.img'.
Load address: 0x81000000
Loading: #################################################T ################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         #################################################################
         ####
done
Bytes transferred = 3014660 (2e0004 hex)

db12x> erase 0x9f020000 +2e0004

First 0x2 last 0x30 sector size 0x10000
  48
Erased 47 sectors

db12x> cp.b 0x81000000 0x9f020000 0x2e0004
Copy to Flash... write addr: 9f020000
done

SIEMENS Gigaset SX763
http://wiki.openwrt.org/toh/gigaset/sx76x 
http://linux.jezgra.net/2013/02/sx763‑hack/ 
serial port enabled
ROM VER: 1.0.3
CFG 04
Read EEPROMX
 X
UART

Now, openwrt wiki points to missing u‑boot.asc but there is one on https://code.google.com/p/sx76x‑openwrt‑danube/source/browse/trunk/u‑boot.asc 
dpavlin@blue:/bluez/openwrt/sx76x$ wget https://code.google.com/p/sx76x-openwrt-danube/source/browse/trunk/u-boot.asc

dpavlin@blue:/bluez/openwrt/sx76x$ cat u-boot.asc > /dev/ttyUSB0