Author: [see doc]
Document comments: generated by HTML::FormatRTFWithImages (v?, using HTML::TreeBuilder v3.130, and HTML::Parser v3.55)

bojler
root@bojler:/sys/class/gpio# ls
 export gpio8 gpiochip0 unexport
 root@bojler:/sys/class/gpio# cat /etc/rc.local
1.. Put your custom commands here that should be executed once
2.. the system init finished. By default this file does nothing.
1.. USB power
echo 0 > /sys/class/gpio/gpio8/value
 echo 1 > /sys/class/gpio/gpio8/value
 dmesg | tail ‑3
/usr/bin/remserial ‑x 2 ‑p 23000 ‑s "9600 raw" /dev/ttyUSB0 &
exit 0
 root@bojler:/sys/class/gpio#