Contents: [Dobrica Pavlinušić's random unstructured stuff]
• Dobrica Pavlinušić's random unstructured stuff (disable secure boot) 
• Dobrica Pavlinušić's random unstructured stuff (Hacking with x86 Windows Tablet and mobile devices on Debian #debconf18) 
• Dobrica Pavlinušić's random unstructured stuff (boot problems) 

Intel Atom Dual Core Z2760 Processor 1.5 GHz (1 MB Cache)
 64 GB Internal Memory, 2 GB RAM Memory
https://www.acer.com/ac/en/ID/content/support‑product/4549 ;‑;
https://wiki.debian.org/InstallingDebianOn/Acer/Iconia_Tab_w500/squeeze 
F2 gets to BIOS, F12 gets boot prompt.
Booted from debian live USB to test, then installed from live USB.
During boot, volume acts as up/down (for grub, bios, etc) and windows button acts as select. power down the system completely
disable secure boot
Connect an external USB DVD drive using the micro USB to female USB adapter.
 Enter the bios by pressing F2 
 Tap on Security and set a Supervisor password.
 Select the Boot page and then Disable Secure Boot.
 Under Boot priority order, use the arrow buttons to set the USB CDROM to the top of the boot priority order.
Hacking with x86 Windows Tablet and mobile devices on Debian #debconf18
https://www.slideshare.net/kapper1224/hacking‑with‑x86‑windows‑tablet‑and‑mobile‑devices‑on‑debian‑debconf18 
https://www.youtube.com/watch?v=RSsgYDfFeHQ 
http://kapper1224.sakura.ne.jp/ 
From presentation it seems that debian multiarch iso should boot and it does. However, installer doesn't start for me
boot problems
• http://www.linuxium.com.au/how‑tos