Contents: [Dobrica Pavlinušić's random unstructured stuff]
• Dobrica Pavlinušić's random unstructured stuff (IM‑ME) 
• Dobrica Pavlinušić's random unstructured stuff (console) 
• Dobrica Pavlinušić's random unstructured stuff (pinout) 
• Dobrica Pavlinušić's random unstructured stuff (flasing using RaspberryPi) 
• Dobrica Pavlinušić's random unstructured stuff (dongle) 
• Dobrica Pavlinušić's random unstructured stuff (rfcat) 
• Dobrica Pavlinušić's random unstructured stuff (links) 

IM‑ME
• http://daveshacks.blogspot.com/2010/01/im‑me‑hacking.html 
• http://travisgoodspeed.blogspot.com/2010/03/im‑me‑goodfet‑wiring‑tutorial.html 
• https://github.com/m0nk/IMME 
console
pinout
• (square pad) RESET_N
• P2_1 = debug data
• P2_2 = debug clock
• +2.5 volts (CC1110 VDD max 3.9V)
• Gnd
Spectrum analyzer https://github.com/mossmann/im‑me 
flasing using RaspberryPi 
git clone https://github.com/tobyjaffey/cctl

pi@raspberrypi ~/cctl $ git diff
diff --git a/ccpil/dbg.c b/ccpil/dbg.c
index 9ca33da..2b4a796 100644
--- a/ccpil/dbg.c
+++ b/ccpil/dbg.c
@@ -30,9 +30,9 @@
 
 #define NUM_ATTEMPTS 100
 
-#define PIN_DD RPI_GPIO_P1_11
-#define PIN_DC RPI_GPIO_P1_12
-#define PIN_RST RPI_GPIO_P1_13
+#define PIN_DD RPI_GPIO_P1_21
+#define PIN_DC RPI_GPIO_P1_23
+#define PIN_RST RPI_GPIO_P1_24

 #define ST_CHIP_ERASE_DONE   0x80

wget https://github.com/mossmann/im-me/raw/master/specan/specan.hex

sudo ./ccpil -f specan.hex

dongle

Mine is different board revision
rfcat
• https://bitbucket.org/atlas0fd00m/rfcat 
links
• https://github.com/mossmann/cc11xx  ‑ Hardware designs for CC11xx
• https://github.com/tobyjaffey/cctl  ‑ ChipCon Tiny Loader, a 1KB serial bootloader for CC1110/CC1111
• https://github.com/samyk/opensesame  ‑ OpenSesame attacks wireless garages and can open most fixed‑code garages and gates in seconds