This page will try to document my experiment to run mainline kernel on OMAP

Contents: [Dobrica Pavlinušić's random unstructured stuff]
• Dobrica Pavlinušić's random unstructured stuff (uart) 

CPU 800 MHz ARM Cortex‑A8‑based TI OMAP3621[1]
 Memory 512 MB
 Storage 8 GB internal
 32 GB max via microSD
 Display 7‑inch 1024 x 600 px WSVGA IPS LCD at 170 ppi
 Graphics PowerVR SGX 530
 Input Capacitive multitouch screen with side volume, Nook Home, and power button
 Connectivity Wi‑Fi 802.11 b/g/n, USB, Bluetooth(Disabled on stock firmware)
 Power Installed battery 3.7 v 4000 mAh (8 hours with Wi‑Fi off)
 Dimensions 8.1 in (210 mm) H
 5.0 in (130 mm) W
 0.48 in (12 mm) D
 Mass 15.8 oz (450 g)
• https://www.xda‑developers.com/patch‑this‑barnes‑and‑noble‑nook‑tablet‑hardware‑protection‑compromised/ 
uart