Author: [see doc]
Document comments: generated by HTML::FormatRTFWithImages (v?, using HTML::TreeBuilder v3.130, and HTML::Parser v3.55)

After four (4) weeks of waiting from the moment credit card has been charged, it finally arrived. It seems that shipping GSM‑like devices to Croatia as person (as opposed to company) isn't something envisioned by Hrvatske agencije za telekomunikacije  so we had to get additional papers (most of which I don't have) and in the end they settled with hardware specification of Neo1973 from OpenMoko wiki.
I must say that people all over the process where helpful and nice: we had to communicate much more with them then I hoped, but in the end it worked out o.k.
And now several obligatory pictures (hopefully not redundant :‑)
http://blog.rot13.org/2007/08/24/openmoko‑goodies.jpghttp://blog.rot13.org/2007/08/24/openmoko‑size.jpghttp://blog.rot13.org/2007/08/24/openmoko‑assembly_required.jpg
After that I got rootfs flashed and I now have new (semi‑functional) phone :‑)

root@fic-gta01:~$ cat /proc/cpuinfo
Processor       : ARM920T rev 0 (v4l)
BogoMIPS        : 132.71
Features        : swp half thumb
CPU implementer : 0x41
CPU architecture: 4T
CPU variant     : 0x1
CPU part        : 0x920
CPU revision    : 0
Cache type      : write-back
Cache clean     : cp15 c7 ops
Cache lockdown  : format A
Cache format    : Harvard
I size          : 16384
I assoc         : 64
I line length   : 32
I sets          : 8
D size          : 16384
D assoc         : 64
D line length   : 32
D sets          : 8

Hardware : GTA01
 Revision : 0240
 Serial : 0000000000000000
 root@fic‑gta01:~$ free
 total used free shared buffers cached
 Mem: 126644 52604 74040 0 84 39100
 ‑/+ buffers/cache: 13420 113224
 Swap: 0 0 0
 root@fic‑gta01:~$ df
 Filesystem 1k‑blocks Used Available Use% Mounted on
 /dev/mtdblock4 62576 42572 20004 68% /
 tmpfs 40 0 40 0% /mnt/.psplash
 /dev/mtdblock4 62576 42572 20004 68% /dev/.static/dev
 tmpfs 2048 64 1984 3% /dev
 tmpfs 63320 4 63316 0% /tmp
 tmpfs 63320 116 63204 0% /var/volatile
 tmpfs 63320 16 63304 0% /dev/shm
 tmpfs 63320 0 63320 0% /media/ram
 /dev/mmcblk0p1 495168 0 495168 0% /media/card