WB3‑12 360 Degree Microwave Motion Detector Module 12V‑35V 
Features:
 Working Voltage: 12V ~ 35V DC
 Quiescent Current: <7mA
 Output Type: Digital
 Default Delay Time: 1S (1~120S adjustment delay, please explain in advance)
 Sensing Distance: 5m ~ 8m (default setting 6 meters)
 Detection Angle: 180� x 360�
 Output Signal: 3.3V , Low: 0V 
 Pin Number: 3 Pins
 Operating Temperature: ‑20�C ~ +80�C
 Size: 17.5mm x 23mm / (round plate D25)
In my testing works on 5V, has 10s delay on trigger.